Feb 05, 2008

If your printer is SOLJET PRO3 XC-540, please note the following.

With this version of Roland VersaWorks, only the Roland original media profiles that support Roland Intelligent Pass Control are installed. If you need to use a Roland original media profile that doesn't support Roland Intelligent Pass Control, please follow the steps below to import the RML files.

[How to Add the RML Files]
1. Start up Roland VersaWorks.
2. Click [Media] – [Media Explorer].
   Media Explorer opens.
3. Click the [Load from File] button.
4. On the [Open] dialogue, select the RML file stored in this folder. Select “XC_EcoMAX_CMYKLcLm.rml” when the ink type you are using is CMYKLcLm and select
“XC_EcoMAX_CMYK.rml” when using CMYK.
5. Click [Open] button.
   The [Import Media] dialogue opens.
6. The list of all the Roland original media profiles is displayed. Select a media you need and click the [OK] button. The selected media is imported to Media Explorer.
7. Click the [OK] button and close Media Explorer.

* The Roland original media profiles cannot be deleted once they are imported. It is recommended to import only the necessary profiles.